**Project Status Report**

|  |  |
| --- | --- |
| **Project Name** | Coded Messaging System |
| **Team Members** | Alan Cranbury, Mark Mahony |
| **Report Date** | November 2, 2012 |

**Project Overall Status: Yellow**

Text message are compressed and sent and uncompressed successfully. Voice is sent, but not played back perfectly. Checksums have been implemented, simple testing for checksums work properly are present. Error detection and correction of receiver ID has been implemented and functions. Sender phonebook is operational and visible.

**Activities – During the Past Week**

|  |  |  |
| --- | --- | --- |
| **Activity** | **Planned Completion Date** | **% Complete** |
| Testing of and debug of final system | Friday, November 9, 2012 | 90% |
| UI Implementation | Friday, November 9, 2012 | 100% |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Activities Planned – For the Next Week**

|  |  |
| --- | --- |
| **Activity** | **Planned Completion Date** |
|  |  |

**Outstanding Issues**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Responsibility** | **Date to be Resolved** | **Proposed Resolution** |
| RS-232 cannot pick up the signal coming from the hardware. | Mark | N/A | Tweak the circuit to work at a lower baud rate. However, the current baud rate is very stable, the deFSK most likely cannot interpret the RS-232 data input. |

**Changes to Plan**

|  |  |  |
| --- | --- | --- |
| **Change** | **Date of Change** | **Impact to Project** |
| N/A |  |  |
|  |  |  |